Cyclone Notes

* For computing EO if ieo\_type=1 then must first be an ellipse emittance entered – this needs to be trapped – add to instructions
* For ieo\_type=1 then is no log file (EO.LOG)
* For ieo\_type=3 the log file includes the data at the gaps
* Appears to be a gap line search issue (currently it stops at the 39 MeV) – needs repair